

**STATIC TO DHCP**





**PURANA KAM BUT SIRF ROUTER PE**


Shorterpath pe jane ky liye we use rip


Dynamic main routers ko wese hi ip assign krte hain sirf host ko nhi krte

















**CREATING DYNAMIC IP**









**PINGING WITHIN THE SAME NETWORK**




**PINGING WITHIN THE DIFFERENT NETWORK**








**PINGING SHOULD BE SUCCESSFUL FOR EVERY CASE**





**SHOW IP ROUTE**

